/*
 * Copyright (c) 2020 The ZMK Contributors
 *
 * SPDX-License-Identifier: MIT
 */

#include <behaviors.dtsi>
#include <dt-bindings/zmk/keys.h>

/* Uncomment and keep whatever encoders are on your BDN9
&sensors {
	status = "okay";
	sensors = <&left_encoder &mid_encoder &right_encoder>;
};
*/

// Uncomment each encoder installed on your BDN9
// &left_encoder { status = "okay"; };
// &mid_encoder { status = "okay"; };
// &right_encoder { status = "okay"; };

/ {
	keymap {
		compatible = "zmk,keymap";

		default_layer {
			bindings = <
				&kp HOME  &kp K_PP &kp END
				&kp PG_UP &kp UP   &kp PG_DN
				&kp LEFT  &kp DOWN &kp RIGHT
			>;
			/* Uncomment and add necessary bindings. This examples is for one encoder
			sensor-bindings = <&inc_dec_kp PG_UP PG_DN>;
			*/
		};
	};
};

